%%%
% Dessin Algo
%%%
\def\filedateDessinAlgo{2025/05/26}%
\def\fileversionDessinAlgo{0.1}%
\message{-- \filedateDessinAlgo\space v\fileversionDessinAlgo}%
%
\newtoks\tokDessinAlgo%
\def\UpdatetoksDA#1\nil{\addtotok\tokDessinAlgo{#1,}}%

\setKVdefault[DessinAlgo]{Solution=false,Largeur=14,Hauteur=14,Origine={(0,0)},Consignes=8,Enonce=false,Code=false,Relatif=false,Symbole,Traces={},Couleur={}}%
\defKV[DessinAlgo]{%
  Traces=\ifempty{#1}{}{\setKV[DessinAlgo]{Code}},%
  Couleur=\ifempty{#1}{}{\setKV[DessinAlgo]{Solution}}%
}%

\NewDocumentCommand\DessinAlgo{om}{%
  \tokDessinAlgo{}%
  \useKVdefault[DessinAlgo]%
  \setKV[DessinAlgo]{#1}%
  \setsepchar[*]{/}\ignoreemptyitems%
  \readlist*\PfCListeDessinAlgo{#2}%
  \reademptyitems%
  \foreachitem\compteur\in\PfCListeDessinAlgo{\expandafter\UpdatetoksDA\compteur\nil}%
  \ifboolKV[DessinAlgo]{Relatif}{%
    \BuildDessinAlgoRelatif{\the\tokDessinAlgo}%
  }{%
    \BuildDessinAlgo{\the\tokDessinAlgo}%
  }%
}%

\NewDocumentCommand\BuildDessinAlgoRelatif{m}{%
    \mplibforcehmode%
    \begin{mplibcode}
      u:=1cm;
      LongueurConsigne=\useKV[DessinAlgo]{Consignes};
      LargeurQuad=\useKV[DessinAlgo]{Largeur};
      HauteurQuad=\useKV[DessinAlgo]{Hauteur};
      pair A[][],B[];
      path zone;
      zone=unitsquare scaled 3.5mm;
      boolean Enonce,Code,Solution,Symbole;
      Enonce=\useKV[DessinAlgo]{Enonce};
      Code=\useKV[DessinAlgo]{Code};
      Solution=\useKV[DessinAlgo]{Solution};
      Symbole=\useKV[DessinAlgo]{Symbole};
      color Couleur;
      if Solution:
      Couleur=\useKV[DessinAlgo]{Couleur};
      fi;
      %
      vardef DessineConsigne(text t)=
      n:=0;
      nborig:=0;
      k=1;
      l:=1;
      %On détermine les points de départs;
      for p_=t:
      if pair p_:
      nborig:=nborig+1;
      if (n mod LongueurConsigne)>0:
      l:=l-1;
      elseif nborig=2:
      l:=l-1;
      fi;
      k:=1;
      n:=0;
      B[nborig]=0.35*u*(k,2*l+0.5);
      else:
      if numeric p_:
      n:=n+1;
      NBorig[nborig]:=n;
      if (n mod 2)=1:
      Deplacement[nborig][(n+1) div 2]=p_;
      else:
      TourneAngle[nborig][n div 2]=p_
      fi;
      fi;
      fi;
      endfor;
      % On affiche
      picture RetiensLong;
      r:=0;
      Long:=0;
      h:=0;
      for k=1 upto nborig:
      if k>1:
      r:=r-2;
      Long:=0;
      h:=0;
      fi;
      for l=1 step 2 until NBorig[nborig]-1:
      if l=1:
      RetiensLong:=image(label.rt(TEX("av "&decimal(Deplacement[k][(l+1) div 2])),(0,0)));
      draw RetiensLong shifted (Long,5mm*r);
      if nborig=1:
      %
      else:
      label.lft(TEX("D$_"&decimal(k)&"$"),(Long,5mm*r));
      fi;% label(TEX(decimal(h)),3.5mm*(0,-h)) withcolor red;
      Long:=Long+abs(lrcorner RetiensLong-llcorner RetiensLong)+1mm;
      h:=h+1;
      else:
      EcartAngle:=TourneAngle[k][(l+1) div 2]-TourneAngle[k][(l-1) div 2];
      if EcartAngle>0:
        if EcartAngle<180:
          if Symbole:
            RetiensLong:=image(
            drawarrow ((point(1) of zone){dir90}..{dir180}(point(3) of zone)) shifted(1mm,-1mm);
            label.rt(TEX("\ang{"&decimal(EcartAngle)&"}"),point(1) of zone);
            );
          else:
            RetiensLong:=image(label.rt(TEX("TG \ang{"&decimal(EcartAngle)&"}"),(0,0)));
          fi;
        else:
          if Symbole:
            RetiensLong:=image(
            drawarrow ((point(0) of zone){dir90}..{dir0}(point(2) of zone)) shifted(1mm,-1mm);
            label.rt(TEX("\ang{"&decimal(360-EcartAngle)&"}"),point(1) of zone);
            );
          else:
            RetiensLong:=image(label.rt(TEX("TD \ang{"&decimal(360-EcartAngle)&"}"),(0,0)));
          fi;
        fi;
      else:
      if abs(EcartAngle)<180:
      if Symbole:
      RetiensLong:=image(
      drawarrow ((point(0) of zone){dir90}..{dir0}(point(2) of zone)) shifted(1mm,-1mm);
      label.rt(TEX("\ang{"&decimal(abs(EcartAngle))&"}"),point(1) of zone);
      );
      else:
      RetiensLong:=image(label.rt(TEX("TD \ang{"&decimal(abs(EcartAngle))&"}"),(0,0)));
      fi;
      else:
      if Symbole:
      RetiensLong:=image(
      drawarrow ((point(1) of zone){dir90}..{dir180}(point(3) of zone)) shifted(1mm,-1mm);
      label.rt(TEX("\ang{"&decimal(360-abs(EcartAngle))&"}"),point(1) of zone);
      );
      else:
      RetiensLong:=image(label.rt(TEX("TG \ang{"&decimal(360-abs(EcartAngle))&"}"),(0,0)));
      fi;
      fi;
      fi;
      draw RetiensLong shifted (Long,5mm*r);
      Long:=Long+abs(lrcorner RetiensLong-llcorner RetiensLong)+1mm;
      %label(TEX(decimal(h)),3.5mm*(0,-h)) withcolor blue;
      RetiensLong:=image(label.rt(TEX("Av "&decimal(Deplacement[k][(l+1) div 2])),(0,0)));
      draw RetiensLong shifted (Long,5mm*r);
      Long:=Long+abs(lrcorner RetiensLong-llcorner RetiensLong)+1mm;
      h:=h+1;
      %label(TEX(decimal(h)),3.5mm*(0,-h)) withcolor green;
      fi;
%      label(TEX(decimal(h mod 8)),3.5mm*(0,-h)) withcolor Purple;
      if ((h mod LongueurConsigne)=0):% and (h>0):
      %label(TEX("OKAYYYYYYY"),3.5mm*(0,-h)) withcolor Purple;
      Long:=0;
     r:=r-1;
      h:=0;
      fi;
      endfor;
      endfor;
      enddef;
      %
      vardef DessinQuadrillage(text t)=
      drawoptions(withcolor 0.7white);
      for k=0 upto LargeurQuad:
      trace (3.5mm*(k,0))--(3.5mm*(k,HauteurQuad));
      endfor;
      for k=0 upto HauteurQuad:
      trace (3.5mm*(0,k))--(3.5mm*(LargeurQuad,k));
      endfor;
      drawoptions();
      % On détermine les points
      n=0;
      nborig:=0;
      for p_=t:
      if pair p_:
      nborig:=nborig+1;
      A[nborig][0]=3.5mm*p_;
      n:=0;
      else:
      n:=n+1;
      NombreOrig[nborig]:=n;
      Nombre[nborig][n]=p_;
      fi;
      endfor;
      for l=1 upto nborig:
      for k=1 step 2 until NombreOrig[l]:
      if (Nombre[l][k+1] mod 90)=0:
      long:=3.5mm
      else:
      long:=sqrt(2)*3.5mm
      fi;
      A[l][(k+1) div 2]-A[l][k div 2]=long*Nombre[l][k]*(unitvector((1,0)-(0,0)) rotated Nombre[l][k+1]);
      endfor;
      endfor;
      if nborig=1:
      dotlabel("",A[nborig][0]);
      label.ulft(TEX("D"),symetrie(A[nborig][1],A[nborig][0]));
      drawarrow A[nborig][0]--(0.75[A[nborig][0],A[nborig][1]]);
      else:
      for k=1 upto nborig:
      label(TEX("D$_"&decimal(k)&"$"),symetrie(A[k][1],A[k][0]));
      dotlabel("",A[k][0]);
      drawarrow A[k][0]--(0.75[A[k][0],A[k][1]]);
      endfor;
      fi;
      enddef;
      %
      vardef DessineSolution=
      for l=1 upto nborig:
      for k=1 step 2 until NombreOrig[l]:
      draw A[l][(k div 2)]--A[l][(k+1) div 2] withpen pencircle scaled 2 withcolor Couleur;
      endfor;
      endfor;
      enddef;
      if Enonce:
      DessineConsigne(#1);
      else:
      DessinQuadrillage(#1);
      if Code:
      \useKV[DessinAlgo]{Traces};
      fi;
      if Solution:
      DessineSolution;
      fi;
      fi;
    \end{mplibcode}
}%

\NewDocumentCommand\BuildDessinAlgo{m}{%
    \mplibforcehmode%
    \begin{mplibcode}
      u:=1cm;
      LongueurConsigne=\useKV[DessinAlgo]{Consignes};
      LargeurQuad=\useKV[DessinAlgo]{Largeur};
      HauteurQuad=\useKV[DessinAlgo]{Hauteur};
      pair A[][],B[];
      path zone;
      zone=unitsquare scaled 3.5mm;
      boolean Enonce,Code,Solution;
      Enonce=\useKV[DessinAlgo]{Enonce};
      Code=\useKV[DessinAlgo]{Code};
      Solution=\useKV[DessinAlgo]{Solution};
      color Couleur;
      if Solution:
      Couleur=\useKV[DessinAlgo]{Couleur};
      fi;
      %
      vardef DessineConsigne(text t)=
      n:=0;
      nborig:=0;
      k=1;
      l:=1;
      for p_=t:
      if pair p_:
      nborig:=nborig+1;
      if (n mod LongueurConsigne)>0:
      l:=l-1;
      elseif nborig=2:
      l:=l-1;
      fi;
      k:=1;
      n:=0;
      B[nborig]=0.35*u*(k,2*l+0.5);
      else:
      n:=n+1;
%      draw (zone shifted(0.35*u*(k,2*l)));
      if (n mod 2)=1:
      label(TEX(decimal(p_)),(center zone) shifted(0.35*u*(k,2*l)));
      k:=k+1;
      else:
      if p_=0:
      drawarrow ((point(0) of (unitsquare scaled 3.5mm))--(point(1) of (unitsquare scaled 3.5mm))) shifted ((center zone) shifted(u*(0.35*k-0.175,0.35*2*l)));
      elseif p_=45:
      drawarrow ((point(0) of (unitsquare scaled 3.5mm))--(point(2) of (unitsquare scaled 3.5mm))) shifted ((llcorner zone) shifted(u*0.35*(k,2*l)));
      elseif p_=90:
      drawarrow ((point(0) of (unitsquare scaled 3.5mm))--(point(3) of (unitsquare scaled 3.5mm))) shifted ((llcorner zone) shifted(u*(0.35*k+0.175,0.35*2*l)));
      elseif p_=135:
      drawarrow ((point(1) of (unitsquare scaled 3.5mm))--(point(3) of (unitsquare scaled 3.5mm))) shifted ((llcorner zone) shifted(u*0.35*(k,2*l)));
      elseif p_=180:
      drawarrow ((point(1) of (unitsquare scaled 3.5mm))--(point(0) of (unitsquare scaled 3.5mm))) shifted ((center zone) shifted(u*(0.35*k-0.175,0.35*2*l)));
      elseif p_=-45:
      drawarrow ((point(3) of (unitsquare scaled 3.5mm))--(point(1) of (unitsquare scaled 3.5mm))) shifted ((llcorner zone) shifted(u*0.35*(k,2*l)));
      elseif p_=-90:
      drawarrow ((point(3) of (unitsquare scaled 3.5mm))--(point(0) of (unitsquare scaled 3.5mm))) shifted ((llcorner zone) shifted(u*(0.35*k+0.175,0.35*2*l)));
      elseif p_=-135:
      drawarrow ((point(2) of (unitsquare scaled 3.5mm))--(point(0) of (unitsquare scaled 3.5mm))) shifted ((llcorner zone) shifted(u*0.35*(k,2*l)));
      fi;
      drawoptions();
      k:=k+2;
      fi;
      if (k mod (2*LongueurConsigne+(LongueurConsigne)+1))>0:
      else:
      l:=l-1;
      k:=1;
      fi;
      fi;
      endfor;
      if nborig=1:
      label.lft(TEX("D"),B[1]);
      else:
      for k=1 upto nborig:
      label.lft(TEX("D$_"&decimal(k)&"$"),B[k]);
      endfor;
      fi;
      enddef;
      %
      vardef DessinQuadrillage(text t)=
      drawoptions(withcolor 0.7white);
      for k=0 upto LargeurQuad:
      trace (3.5mm*(k,0))--(3.5mm*(k,HauteurQuad));
      endfor;
      for k=0 upto HauteurQuad:
      trace (3.5mm*(0,k))--(3.5mm*(LargeurQuad,k));
      endfor;
      drawoptions();
      % Les points
      n=0;
      nborig:=0;
      for p_=t:
      if pair p_:
      nborig:=nborig+1;
      A[nborig][0]=3.5mm*p_;
      n:=0;
      else:
      n:=n+1;
      NombreOrig[nborig]:=n;
      Nombre[nborig][n]=p_;
      fi;
      endfor;
      for l=1 upto nborig:
      for k=1 step 2 until NombreOrig[l]:
      if (Nombre[l][k+1] mod 90)=0:
      long:=3.5mm
      else:
      long:=sqrt(2)*3.5mm
      fi;
      A[l][(k+1) div 2]-A[l][k div 2]=long*Nombre[l][k]*(unitvector((1,0)-(0,0)) rotated Nombre[l][k+1]);
      endfor;
      endfor;
      %
      if nborig=1:
      dotlabel.ulft(TEX("D"),A[nborig][0]);
      else:
      for k=1 upto nborig:
      dotlabel.ulft(TEX("D$_"&decimal(k)&"$"),A[k][0]);
      endfor;
      fi;
      enddef;
      %
      vardef DessineSolution=
      for l=1 upto nborig:
      for k=1 step 2 until NombreOrig[l]:
      draw A[l][(k div 2)]--A[l][(k+1) div 2] withpen pencircle scaled 2 withcolor Couleur;
      endfor;
      endfor;
      enddef;
      if Enonce:
      DessineConsigne(#1);
      else:
      DessinQuadrillage(#1);
      if Code:
      \useKV[DessinAlgo]{Traces};
      fi;
      if Solution:
      DessineSolution;
      fi;
      fi;
    \end{mplibcode}
}%